**Handheld Viewer Operation**

1. For best results, darken room and provide a black background 6-8 inches (150-200mm) below cell.
2. Turn on power switch.
3. Hold viewer with switch facing down.
4. Place magnet on top of glass cell.
5. Leave in position until image manifests.
6. Rotate & flip magnet position to see other aspects of field.

Alternately:

1. Place plastic magnet stand on flat surface with black background.
2. Place magnet on top of stand.
3. Move viewer glass down close- almost touching magnet.
4. Hold in position until image manifests.
5. Move viewer away and rotate magnet position.
6. Notice now the field has changed with the magnets orientation.

**Wait 10-30 seconds for the image to manifest. Move magnets position often.**

**Resting magnet in one position for long periods of time may burn the inside surface of the glass, creating a blurred view in the affected area.**

 **Battery removal:**

 ****

Slide cover away from cell

Lift end of battery holder from handle

Slide top cover toward cell.

Remove and recharge batteries.

Repeat procedure in reverse after charging.

**Battery charger info:**

Insert battery into charger slot with (-) end facing USB plug.

Set (+) in first and firmly press in (–) last. Remove in opposite order: (-) end first.

Recharge time for both batteries is approx. 55 hours from complete discharge of cells.